{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["ML307A_BOM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ML307A_BOM","index":0,"n_rows":91,"n_cols":7,"rows_kept":91,"cut":false,"hidden":false,"merged":[[89,6,90,6]]}
["  Revised: Monday, December 19, 2022"]
["          Revision: "]
{"$rows_empty":7}
["Bill Of Materials        January 3,2023      9:01:00","Page1"]
[]
["Item","Quantity","Reference","Part","PCB Footprint","特性备注","推荐品牌"]
["______________________________________________"]
[null,{"$f":"SUM(B15,B16,B17,B18,B19,B20,B21,B22,B23,B24,B26,B27,B28,B32,B39,B41,B40,B42,B43,B44,B45,B46,B49,B50,B51,B53,B54,B55,B56,B57,B59,B61,B62,B63,B66,B70,B71,B72,B73,B75,B74,B76,B78,B79,B80,B81,B82,B83,B84,B85,B87,B88,B90,B91)","v":118}]
[1,1,"ANT","30mm专用天线焊接点","PAD1_5mm_h09"]
[2,2,"CV1,CV2","470uF ±20% 6.3V","smd6_3x7_7","重要器件","KNSCHA(科尼盛)"]
[3,9,"C2,CV5,C18,C21,C22,C144,C29,C31,C34","1uF ±10% 16V","C0402"]
[4,4,"CV6,C13,C143,C139","4.7uF ±10% 10V","C0402"]
[5,1,"CV7","100uF 10V","SMD_5X5.4","重要器件","KNSCHA(科尼盛)"]
[6,1,"CV8","2FL/3V8","DIP2_54mm","关键器件","中科超容"]
[7,4,"C3,C4,C7,C8","33pF ±5% 50V   C0G","C0402"]
[8,4,"C5,C6,C14,C15","NC","C0402"]
[9,1,"C11","2.2uF ±20% 10V","C0402"]
[10,6,"C12,C19,C20,C23,C24,C37","100nF ±10% 25V","C0402"]
[]
[12,2,"C16,C17","10pF ±5% 50V C0G","C0402"]
[13,5,"C26,C27,C48,C125,C127","22uF ±20% 25V","C0805"]
[14,2,"C28,C30","6pF ±0.25pF 50V  C0G","C0402"]
[]
[]
[]
[18,1,"C126","10uF ±20% 16V","C0603"]
[]
[]
[]
[]
[]
[]
[23,3,"D1,D2,D6","红灯 617.5nm发光二极管/LED","L0603"]
[24,3,"D4,D8,D19","ESD5302F","SOT23"]
[25,2,"D7,D13","LM2904","so8","重要器件","友顺//友台"]
[26,2,"D10,D14"," SMF12CA","sod123"]
[27,2,"D12,D17","GBLC05","SOD-323"]
[28,1,"D15"," SMF15CA","sod123"]
[29,1,"D16","B5817WS","SOD-323","关键器件","长电"]
[30,1,"D18","1N4148WS","SOD-323"]
[]
[]
[33,1,"L1","4.7uH ±20% 700mA 500mΩ\n功率电感","R0603","关键器件","风华"]
[34,2,"L2,R4","0Ω","R0402"]
[null,1,"R54","NC"]
[]
[37,4,"Q1,Q2,Q3,Q5","SS8050","SOT-323","重要器件","长电"]
[38,1,"Q4","NDS352AP P沟道 30V 5.6A\n","SOT-23","重要器件","微碧"]
[39,1,"Q6","LM317 正 Vout=1.2V~37V 2.2A","sot-223n","关键器件","友台 友顺 其他品牌则电流不低于1.5A"]
[40,3,"RL1,RL2,R17","2K 1%","R0402"]
[41,4,"RL5,RL6,RL7,RL13","1K 5%","R0402"]
[]
[43,10,"R2,RL8,R36,R37,R38,R46,R16,R55,R62,R63","10K","R0402"]
[]
[44,2,"RL9,RL11","3K","R0402"]
[45,2,"RL10,RL12","12K","R0402"]
[46,3,"RP1,R49,R50","100Ω","R0402"]
[]
[]
[48,5,"R3,R5,R6,R52,R53","22Ω","R0402"]
[]
[]
[]
[52,1,"R19","10K/NTC 0805","R0805"]
[53,2,"R22,R30","0Ω","R0603"]
[54,1,"R39","133Ω","R0402"]
[55,1,"R40","249Ω","R0402"]
[56,1,"R44","510Ω","R0603"]
[57,1,"R45","1Ω","R0603"]
[58,1,"R51","5.1Ω","R0805"]
[]
[60,1,"U1","ML307A","LGA-94"]
[61,1,"U01","CN809S","SOT-23","关键器件","上海如韵"]
[null,2,"V1,V2","2N7002W","SOT-323",null,"长电"]
[63,1,"U3"," IPEX-1 贴片天线座 ","SMD"]
[64,1,"U4","ESIM","ESIM_IC-S"]
[65,1,"U8","RTL8762","QFN40"]
[66,1,"U9","LD1117AG-33-AB3-A-R","sot-89","关键器件","友顺 其他品牌 电流不低于500mA"]
[67,1,"U10","BL5372","sop-8"]
[]
[69,1,"U15","NC","miniusb_dip"]
[70,1,"U25","LP3986-18B3F 输入6V 输出1.8V~1.8V 300mA","SOT23"]
[]
[72,1,"Y1","40MHz ±10ppm 10pF -40℃——+85℃","x4-3225",null,"HD(浩都频率) 千芯科技 星通时频，爱普生"]
[73,1,"Y2","32.768kHz ±20ppm 7pF-40℃——+85℃","SMD3215","关键器件"]