{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["NEMA_PWR_BOM_2023"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"NEMA_PWR_BOM_2023","index":0,"n_rows":103,"n_cols":10,"rows_kept":103,"cut":false,"hidden":false,"merged":[[79,0,79,16383],[100,0,101,16383],[102,0,103,4]]}
["  Revised: Tuesday, February 28, 2023"]
["          Revision: "]
{"$rows_empty":7}
["Bill Of Materials          March 3,2023      9:28:14","Page1"]
[]
["Item","Quantity","Reference","Part","PCB Footprint"]
["______________________________________________"]
[]
[]
[2,1,"B1","整流桥 MB10S 1KV 1A(或0.8A）","MBS"]
[]
[4,3,"CM1,CM2,CM12","1UF/25V X7R电容","C0402"]
[5,1,"CM11","10UF/16V X7R电容","C0402"]
[6,4,"CM13.CP7,CP11,CP12","10UF/25V X7R电容","C0603"]
[7,2,"CM14,CP10","1UF/25V X7R电容","C0603"]
[]
[9,1,"CP4","1NF/1KV X7R电容","C1206"]
[10,1,"CP5","102/50V X7R电容","C0603"]
[11,1,"CP6","103/1KV X7R电容","C1206"]
[]
[]
[]
[]
[16,1,"CP22","103/630V X7R电容","C0805"]
[17,1,"CP27","22UF/25V X7R电容","C0805"]
[18,2,"CX1,CX2","20PF/25V  C0G 电容","C0402"]
[]
[20,4,"C9,C10,C30,C31","33NF/25V X7R电容","C0402"]
[21,2,"DL1,DP6","1N4148 二极管","sod-323"]
[22,1,"DP1","SS310 肖特基二极管","SMA",null,null,"关键器件"]
[23,2,"DP2，DP3","1N4007 整流二极管","sod123"]
[]
[25,1,"D1,D2","LED_GREEN 绿光贴片LED","D0603"]
[]
[27,1,"D3","15V 双向TVS管 SMF15CA","SOD123",null,null,"重要器件"]
[28,2,"D4,D5","12V 双向TVS PTVSHC3D12VU  ","SOD-323"]
[]
[]
[]
[]
[]
[34,1,"QL1","SS8050","sot-323",null,null,"重要器件"]
[35,1,"R-100","0R电阻 （与J4保护模块2选1）","R1206"]
[]
[37,1,"RL1","20R ","R0603"]
[38,7,"RL2,R7,R8,R16,R17，RM3,RM5","1K 1%","R0402"]
[39,1,"RM2","10R","R0603"]
[]
[41,2,"RP1,RP6","470K ","R0805"]
[42,1,"RP2","100R","R0603"]
[]
[44,1,"RP4","3K","R0603"]
[45,1,"RP5","100 R","R0805"]
[46,1,"RP7","4R7","R0805"]
[47,1,"RP8","24K","R0603"]
[48,1,"RP9","68K","R0603"]
[49,1,"RP10","4K3","R0603"]
[50,1,"RP11","1R","R1206"]
[51,3,"R9,RP14,RP15","100K","R1206"]
[52,1,"RP18","100R","R1206"]
[]
[54,2,"R5,R6","100 R","R0402"]
[55,2,"R10,RP3","120K","R1206"]
[56,2,"R14,R15","5.1 R","R0402"]
[]
[]
[]
[]
[61,1,"U1","OB2512RN  电源芯片","sop-7"]
[62,1,"U2","RN8209C 计量芯片","SOP16"]
[]
[64,1,"Y1","3.579MH 晶振 -40℃——+85℃20pf","HC-49 SMD",null,null,"关键器件",null," TAITIEN(泰艺电子)或\n千芯科技"]
[]
["                                                      以下为插件器件。"]
[null,2,"CP9,CP8","470UF/25V 电解电容","8X12mmX3.5mm 指定尺寸，不能代用混用",811,null,"重要器件"]
[null,1,"CY2","222/400V   Y1电容","脚距10mm",1107]
[]
[null,1,"U01","电流互感器ZMCT103C","DIP",815,null,"重要器件",null,"择明 "]
[]
[null,1,"CA1","X1 电容 150NF/440V 脚距10mm",null,1107,null,"关键器件"]
[null,1,"RV1","20D681K压敏电阻 6.5KA","DIP"]
[63,1,"U12","电压互感器 2mA:2mA隔离电压4KV。( HPT225HN 或者ZMPT107-5\n）","DIP-4",303,null,"关键器件",null,"择明，霍远"]
[null,1,"AC1---AC2","互感器采样穿管线，1平方毫米，两头剥皮浸锡各3mm，总长60mm",null,815]
[null,1,"CP1","12UF/400V 高压电解电容","8X12mmDIP",811,null,null,null,"艾华"]
[{"$nulls":7},"关键器件"]
[]
[null,2,"LP2,LP4","色环/插件电感 / 470uH ±10% 126mA 7.7Ω","0.25瓦 ",1107,null,"重要器件"]
[null,1,"T1","反激变压器 定制","6脚",815]
[null,1,"RLY1","HF32F-G012-HS 继电器","4脚封装 12V驱动电压",815,null,"重要器件",null,"宏发"]
[null,2,"J1,J2","2.54间距排针4针",null,815]
[null,1,"J4 ","高压保护模块 与R-100电阻2选1","4P特殊固定封装",303]
[null,1,"J3","2.54间距排针3针",null,815]
[null,1,"PCB ","68X68mm 1.6mm无铅喷锡，绿油白字，盖过孔","POWER-S-3.0 2023-2-28",1107]
[null,2]
["注：所有无元件安装的通孔位置，均为后道焊接引线及排针等工序所必需的通孔，需要采取措施给予保留原状。（2021年6月10日注）。"]
[]
["2023年228更新版本：取消隔离电源模块，取消阻容电源，电流和电压采样均采用互感器方式"]